|  |  |  |
| --- | --- | --- |
| Product: | 28-321 | G:\EVP info\Produktinformation - standardsortimentet\Kapsylbilder\EH\321-28 Öppen.JPGG:\EVP info\Produktinformation - standardsortimentet\Kapsylbilder\EH\321-28 Stängd.JPG  |
| Article number: | Please contact our sales department. |
| Product Description: | 28mm Flip-top closure with groove deck adapted for P28-thread.  |
| **Technical specifications** |
| Drawings: | Product drawing: S 28-321Neck drawing: H 321  |
| Sealing: | Ring seal  |
| Plastic resin: | PPH |
| Master batch: | Please contact our sales department. |
| Recommended capping torque: | 1,7-2,0 Nm |
| Storage durability: | 1 year, keep room temperatured in tightly sealed cardboard boxes.  |
| **Quality Control** |
| Standards and norms | Sampling procedure: SS 020130-ISO2859 normal 1Defect classes according to KP-002  |
| **Delivery** |
| Packaging | 2 800 pcs packed in plastic bag packed in cardboard boxes 82dm3. Labels on the boxes. 16 boxes on each pallet with stretch film wrapped around. |
| Traceability | Marking for traceability contains EVP article number, customer article number, production order number, pieces per carton, EVP order number customer order number and date and signature. |