|  |  |  |  |
| --- | --- | --- | --- |
| Product: | | 28-321 | G:\EVP info\Produktinformation - standardsortimentet\Kapsylbilder\EH\321-28 Öppen.JPGG:\EVP info\Produktinformation - standardsortimentet\Kapsylbilder\EH\321-28 Stängd.JPG |
| Article number: | | Please contact our sales department. |
| Product Description: | | 28mm Flip-top closure with groove deck adapted for P28-thread. |
| **Technical specifications** | | |
| Drawings: | | Product drawing: S 28-321 Neck drawing: H 321 | |
| Sealing: | | Ring seal | |
| Plastic resin: | | PPH | |
| Master batch: | | Please contact our sales department. | |
| Recommended  capping torque: | | 1,7-2,0 Nm | |
| Storage durability: | | 1 year, keep room temperatured in tightly sealed cardboard boxes. | |
| **Quality Control** | | | |
| Standards and norms | | Sampling procedure: SS 020130-ISO2859 normal 1  Defect classes according to KP-002 | |
| **Delivery** | | | |
| Packaging | 2 800 pcs packed in plastic bag packed in cardboard boxes 82dm3. Labels on the boxes. 16 boxes on each pallet with stretch film wrapped around. | | |
| Traceability | Marking for traceability contains EVP article number, customer article number, production order number, pieces per carton, EVP order number customer order number and date and signature. | | |