|  |  |  |  |
| --- | --- | --- | --- |
| Product: | | 22-939 UT | 939-22 grön |
| Article number: | | Please contact our sales department. |
| Product Description: | | 22mm closure in HDPE with liner adapted for P22 thread. |
| **Technical specifications** | | |
| Drawings: | | Product drawing: S22-939 O HDPE  Neck drawing: H 939 O | |
| Sealing: | | EPE/PET | |
| Plastic resin: | | HDPE | |
| Master batch: | | Please contact our sales department. | |
| Recommended  capping torque: | | 0,8-1,2Nm | |
| Recommended storage conditions and time for the packaging material | | Temperature:  15-30°C (if the products is being stored under or over temperature conditions they must be stored between 15-30°C for 24 hours before processing  Humidity:  30-70% | |
| Shelf life: | | Wadded components to be used within 12 months counted from manufacturing date. | |
| Food Contact | | Please contact our quality manager for more information. | |
| **Quality Control** | | | |
| Standards and norms | | Sampling procedure: SS 020130-ISO2859 normal 1  Defect classes according to KP-002 | |
| **Delivery** | | | |
| Packaging | 4000 pcs packed in plastic bag, packed in cardboard boxes 45dm3. Labels on the boxes. 24 boxes on each pallet with stretch film wrapped around. | | |
| Traceability | Marking for traceability contains EVP article number, customer article number, production order number, pieces per carton, EVP order number customer order number and date and signature. | | |