|  |  |  |
| --- | --- | --- |
| Product: | 22-939 UT  | 939-22 grön |
| Article number: | Please contact our sales department. |
| Product Description: | 22mm closure in HDPE with liner adapted for P22 thread.  |
| **Technical specifications** |
| Drawings: | Product drawing: S22-939 O HDPE Neck drawing: H 939 O |
| Sealing: | EPE/PET |
| Plastic resin: | HDPE |
| Master batch: | Please contact our sales department. |
| Recommended capping torque: | 0,8-1,2Nm  |
| Recommended storage conditions and time for the packaging material | Temperature: 15-30°C (if the products is being stored under or over temperature conditions they must be stored between 15-30°C for 24 hours before processingHumidity:30-70% |
| Shelf life: | Wadded components to be used within 12 months counted from manufacturing date.  |
| Food Contact  | Please contact our quality manager for more information.  |
| **Quality Control** |
| Standards and norms | Sampling procedure: SS 020130-ISO2859 normal 1Defect classes according to KP-002  |
| **Delivery** |
| Packaging | 4000 pcs packed in plastic bag, packed in cardboard boxes 45dm3. Labels on the boxes. 24 boxes on each pallet with stretch film wrapped around.  |
| Traceability | Marking for traceability contains EVP article number, customer article number, production order number, pieces per carton, EVP order number customer order number and date and signature. |