|  |  |  |
| --- | --- | --- |
| Product: | 40-985/901G | G:\EVP info\Ritningar, e-drawings mm\Kapsylbilder\Standard\BS\901G blå.JPG |
| Article number: | Please contact our sales department. |
| Product Description: | 40mm child resistant closure with liner adapted for P40-thread. |
| **Technical specifications** | |
| Drawings: | Product drawing: S 40-985BS\_00-901G Neck drawing: H 985BS | |
| Sealing: | Liner: EPE/PET | |
| Plastic resin: | Cover: HDPE Closure: HDPE | |
| Master batch: | Please contact our sales department. | |
| Recommended capping torque: | 2,5-3,0Nm | |
| Storage durability: | 1 year, keep room temperatured in tightly sealed cardboard boxes. | |
| Certificate | ZERT 06951530614-8317  The package can only be designated as child resistant and suitable for adults if certified package are used according to ISO 8317. | |
| **Quality Control** | | |
| Standards and norms | Sampling procedure: SS 020130-ISO2859 normal 1  Defect classes according to KP-002 | |
| **Delivery** | | |
| Packaging | 1.600 pcs packed in plastic bag, packed in cardboard boxes 82dm3. Labels on the boxes. 16 boxes on each pallet with stretch film wrapped around. | |
| Traceability | Marking for traceability contains EVP article number, customer article number, production order number, pieces per carton, EVP order number customer order number and date and signature. | |