|  |  |  |
| --- | --- | --- |
| Product: | 00-228  | G:\EVP info\Ritningar, e-drawings mm\Kapsylbilder\Standard\Övrigt\228-00.JPG |
| Article number: | Please contact our sales department. |
| Product Description: | Handle |
| **Technical specifications** |
| Drawings: | Product drawing: S00-228 |
| Sealing: | - |
| Plastic resin: | HDPE |
| Master batch: | Please contact our sales department. |
| Recommended capping torque: | - |
| Storage durability: | 1 year, keep room temperatured in tightly sealed cardboard boxes.  |
| **Quality Control** |
| Standards and norms | Sampling procedure: SS 020130-ISO2859 normal 1Defect classes according to KP-002  |
| **Delivery** |
| Packaging | 24 000 pcs packed in plastic bag, packed in plastic container 1200x800x970mm. The plactic containers shall be returned to EVP. |
| Traceability | Marking for traceability contains EVP article number, customer article number, production order number, pieces per carton, EVP order number customer order number and date and signature. |